{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["技术要求"],"not_rendered":{"external_links":3,"defined_names":25},"read":"whole","date_system":"1900"}

{"sheet":"技术要求","index":0,"n_rows":27,"n_cols":9,"rows_kept":27,"merged":[[0,0,0,6],[1,0,1,6],[2,4,2,6],[3,4,3,6],[4,3,4,6],[5,3,5,6],[6,3,6,6],[7,3,7,6],[8,3,8,6],[9,3,9,6],[10,3,10,6],[11,3,11,6],[12,3,12,6],[13,3,13,6],[14,3,14,6],[15,3,15,6],[16,3,16,6],[17,3,17,6],[18,3,18,6],[19,3,19,6],[20,3,20,6],[21,3,21,6],[22,3,22,6],[23,3,23,6],[24,3,24,6],[25,3,25,6],[26,0,26,6]]}
["视觉检测系统技术要求"]
["设备名称：视觉检测"]
["部门","设备","工艺技术","生产","安徽豪美汽车零部件有限责任公司"]
["审核"]
["序号","评标分类","项目","招标要求"]
[1,"设备能力","柔性生产","检测机器人夹持产品送入安装有固定2D相机的检测室内进行全尺寸视觉识别检测，不同的产品通过更换不同的夹持夹具来实现柔性化检测"]
[2,"设备能力","检测范围","安徽豪美现有芜湖凌云客户67款产品（吸能盒和底板等，具体见清单）"]
[3,"设备能力","检测能力","被检测产品长度≤600mm，重量＜3kg"]
[4,"设备能力","生产节拍","节拍≤21秒/件"]
[5,"设备能力","装夹方式","上料机器人通过吸盘方式（根据产品不同配置1-2个吸盘）、检测机器人通过夹持方式（前期67款产品需配好更换的夹头）"]
[6,"设备能力","工作站尺寸","6600*3000*2200"]
[7,"设备能力","夹具快速换型时间","≤10分钟"]
[8,"检测能力","检测精度","三坐标对比数据误差＜0.08mm"]
[9,"工业机器人","上料","埃斯顿国产机器人1台，载荷20kg以上"]
[10,"工业机器人","检测","埃斯顿国产机器人1台，载荷20kg以上"]
[11,"视觉检测","上料","梅卡曼德3D引导相机LSR L"]
[12,"视觉检测","检测","海康威视2000万像素工业相机"]
[13,"系统集成","PLC系统","西门子1200系列，不能加时间锁，密码锁"]
[14,"系统集成","显示器","32英寸三星彩色液晶显示屏"]
[15,"安全","安全防护","工作站四周全封闭（安全栅栏+安全连锁门开关）"]
[16,"安全","安全防护","急停按钮覆盖所有工位"]
[17,"布局","布局图","提供设备布局图纸"]
[18,"资料","设备资料","提供中文操作手册、电气图纸、PLC和机器人程序源码、易损件清单",{"$nulls":4},"          "]
[19,"培训","培训","现场对生产、工艺、设备为期一周的培训"]
[20,"服务","陪产","至少3个月陪产；期间：1.能够让生产人员独立操作运行生产；2.教会工艺人员调整机器人点位及拉弯机换模等；3.保障维修人员对设备常见问题的解决。"]
[21,"服务","服务","整线质保2年(随时电话响应，24小时现场支持）"]
["所有技术问题可以进行面谈，电话沟通"]