{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["拖车钩类"],"read":"whole","date_system":"1900"}

{"sheet":"拖车钩类","index":0,"n_rows":34,"n_cols":6,"rows_kept":34,"merged":[[0,0,0,6],[1,0,1,6],[2,1,2,2],[2,5,2,6],[3,1,3,2],[3,5,3,6],[4,3,4,6],[5,3,5,6],[6,3,6,6],[7,3,7,6],[8,3,8,6],[9,3,9,6],[10,3,10,6],[11,3,11,6],[12,3,12,6],[13,3,13,6],[14,3,14,6],[15,3,15,6],[16,3,16,6],[17,3,17,6],[18,3,18,6],[19,3,19,6],[20,3,20,6],[21,3,21,6],[22,3,22,6],[23,3,23,6],[24,3,24,6],[25,3,25,6],[26,3,26,6],[27,3,27,6],[28,3,28,6],[29,3,29,6],[30,3,30,6],[31,3,31,6],[32,3,32,6],[33,1,33,6]]}
["拖车钩类视觉检测技术要求"]
["设备名称：拖车钩视觉检测机"]
["部门","设备",null,"生产","工艺","安徽豪美汽车零部件有限责任公司"]
["审核"]
["序号","评标分类","项目","招标要求"]
[1,"功能","控制器系统","厂家成熟系统，系统不能加密码锁、时间锁"]
[2,"检测速度","检测速度","360-500个/小时，检测节拍10秒以内"]
[3,"尺寸测量精度","尺寸测量精度","对被检测物体的尺寸长度、外径、内径达到规定的精度标准"]
[4,"运行稳定性","运行稳定性","需能够7*24小时不间断运行，保证生产的连续性"]
[5,"数据准确性","数据准确性","检测结果要准确可靠，误报率和漏保率要低于2%，不能误将合格产品判定为不合格，也不能放过有缺陷的产品"]
[6,"系统容错性","系统容错性","具备一定的容错能力，当遇到短暂的信号干扰、数据传输故障等问题时，能自动恢复或进行相应处理，不影响整体检验工作"]
[7,"检测项目","检测项目","1、螺纹通规通\n2、螺纹止规止\n3、孔内残屑识别\n4、同轴度和孔径检测                                         \n5、有无烂牙  \n6、有无螺纹"]
[8,"检测产品","产品图档","按豪美工艺技术员提供的产品清单"]
[9,"运行","检测方式","转盘式及通过式"]
[10,"电器","视觉","品牌：康佳或海康或基恩士，如能满足检测需求可放宽品牌限制"]
[11,"上料方式","上料方式","自动上料"]
[12,"下料方式","下料方式","采用料盘，链接包装岗位"]
[13,"电器","电器","施耐德"]
[14,"设计","设计方案","有完整的设计方案（详述针对本项目检测需求的解决方案，包括视觉选型、打光方案、机械设计思路等）"]
[15,"案例","案例","提供至少2个类似零部件视觉检测相关成功案例"]
[16,"公司规模","公司规模","有强大的技术设计队伍，有强大的本工厂工程技术人员及施工技术员"]
[17,"视觉系统","工业相机","高分辨率CCD/CMOS相机（至少500万像素以上），部分检测项目需使用3D激光轮廓仪或3D结构光相机"]
[18,"视觉系统","工业镜头","高分辨率、低畸变远心镜头或普通工业镜头，根据视场和精度选型"]
[19,"视觉系统","光源系统","组合式LED光源（背光、穹顶光、条形光、同轴光等），确保打光方案能突出被测特征，抑制环境光干扰，光源需亮度可调且寿命长"]
[20,"控制系统","工业计算机","工业级工控机（IP从），高性能多核处理器，大容量内存（≥16GB），固态硬盘（SSD），独立显卡（GPU加速可选），预装视觉处理软件"]
[21,"分拣装置","执行机构","与PLC通信，驱动气动或电动执行机构，对NG品进行自动分拣下线进入不良品框"]
[22,"存储功能","数据记录","记录所有产品的检测结果、图像数据（尤其是NG图像），可存储不少于1年"]
[23,"日志功能","系统记录","记录系统操作、报警、错误信息"]
[24,"程序切换","配方管理","支持不同型号产品的检测程序（配方）一键切换"]
[25,"环境适应功能","环境适应性","能适应工业现场环境（振动、粉尘、光照变化等），防护等级不低于IP54"]
[26,"培训","培训","现场对生产、工艺、设备为期一周的培训"]
[27,"服务","陪产","至少15天陪产；期间：1.能够让生产人员独立操作运行生产；2.保障维修人员对设备常见问题的解决"]
[28,"服务","服务","整机保修2年(随时电话响应，能够提供远程支持，48小时现场支持）"]
[null,"所有技术问题可以进行面谈，电话沟通"]