{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["分部分项工程清单表"],"read":"whole","date_system":"1900"}

{"sheet":"分部分项工程清单表","index":0,"n_rows":70,"n_cols":8,"rows_kept":70,"merged":[[0,0,0,7],[1,0,1,4],[1,5,1,7],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,4,3,4],[2,5,2,7],[4,1,4,2],[9,1,9,2],[10,1,10,2],[16,1,16,2],[17,1,17,2],[21,1,21,2],[22,1,22,2],[25,1,25,2],[26,1,26,2],[40,1,40,2],[41,1,41,2],[44,1,44,2],[45,1,45,2],[49,1,49,2],[50,1,50,2],[53,1,53,2],[58,1,58,2],[64,1,64,2],[70,0,70,7]]}
["分部分项工程清单表"]
["工程名称：豪美技术中心卫生间土建工程"]
["序号","项目名称","项目特征描述","计量\n单位","工程数量","金额（元）"]
[{"$nulls":5},"综合单价","合价","品牌备注"]
[null," 拆除及土石方工程"]
[1,"拆除工程","1.原卫生间拆除","项"]
[2,"挖基坑土方","1.土壤类别:按地质报告\n2.挖土深度:2m以内","m3"]
[3,"回填方","1.回填土 夯实机夯实 槽、坑","m3"]
[4,"余方弃置","1.废弃料品种:余土\n2.运距:10km","m3"]
[null,"【土石方工程】分部小计"]
[null," 混凝土及钢筋混凝土工程"]
[5,"独立基础","1.混凝土种类:C25商品混凝土\n2.混凝土强度等级:20石","m3"]
[6,"垫层","1.混凝土种类:C15商品混凝土\n2.混凝土强度等级:20石","m3"]
[7,"基础框架梁、柱、板、圈梁、过梁","1.混凝土种类:C25商品混凝土\n2.混凝土强度等级:20石","m3"]
[8,"现浇构件钢筋","1.钢筋种类、规格:现浇构件带肋钢筋 φ10以内 三级钢","t"]
[9,"现浇构件钢筋","1.钢筋种类、规格:现浇构件带肋钢筋 φ25以内 三级钢","t"]
[null,"【混凝土及钢筋混凝土工程】分部小计"]
[null," 砌筑工程"]
[10,"砌块墙","1.砌块品种、规格、强度等级：200厚蒸压加气混凝土砌块,MU10\n2.墙体类型：外墙\n3.砂浆强度等级：M5.0混合砂浆","m3"]
[11,"砌块墙","1.砌块品种、规格、强度等级：200厚蒸压加气混凝土砌块,MU10\n2.墙体类型：内墙\n3.砂浆强度等级：M5.0混合砂浆","m3"]
[12,"水厕(蹲位)","1.零星砌砖名称、部位:水厕(蹲位)","个"]
[null,"【砌筑工程】分部小计"]
[null," 门窗工程"]
[13,"门","无"]
[14,"深灰色铝白玻璃推拉窗","1.窗类型:深灰色铝白玻璃推拉窗\n2.玻璃品种、厚度、五金材料、品种、规格:1.4mm厚铝合金型材，6厚钢化白玻璃","m2"]
[null,"【门窗工程】分部小计"]
[null," 楼地面装饰工程"]
[15,"地坪（首层）","1.地坪厚度:15cm\n2.混凝土强度等级:C25、20石\n","m2"]
[16,"块料楼地面","1.找平层厚度、砂浆配合比:20厚1:2.5水泥砂浆找平层\n2.面层材料品种、规格、颜色:600×600防滑砖","m2"]
[17,"内外墙面一般抹灰","1.墙体类型：内外墙面\n2.底层厚度、砂浆配合比：20厚1:1:6水泥石灰砂浆底层         3.部位：瓷砖顶及以上\n","m2"]
[18,"内墙面抹灰面油漆","1.油漆品种、刷漆遍数：墙面刮塑白色                     2. 内墙部位：瓷砖顶及以上","m2"]
[19,"外墙面抹灰面油漆","1.基层类型：抹灰底\n2.油漆品种、刷漆遍数：墙面刮塑白色打底 喷白色真石漆","m2"]
[20,"天棚抹灰面油漆","1.基层类型：混凝土板底     2.油漆品种、刷漆遍数：天棚刮塑白色 天棚","m2"]
[21,"内墙面瓷砖","1.基层类型：抹灰底\n2.面层材料品种、规格、颜色:200×400瓷砖           3.高度: 2m","m2"]
[23,"卫生间成品隔断","12mm抗倍特1400密度﹢不锈钢配件","m2"]
[24,"蹲便器","含冲水箱、辅材等","座"]
[25,"小便器","感应小便器","座"]
[null,"洗手盆+25M花岗岩台板"]
[null,"五金水龙头及配件"]
[26,"墙、柱面钉(挂)钢(铁)网 铁丝网","1.墙、柱面钉(挂)钢(铁)网 铁丝网","m2"]
[null,"【装饰工程】分部小计"]
[null,"屋面工程"]
[27,"屋面","1.部位:不上人屋面\n2.找平层材料、厚度:20厚1:2.0水泥砂浆找平层\n3.防水涂料材料、厚度:1.5厚聚氨酯防水涂料\n4.面层材料、厚度:20厚1:2.0水泥砂浆表面压光","m2"]
[28,"变形缝盖板","1.部位：新旧建筑变形缝     2. 盖板：304不锈钢盖板1.0厚    ","m"]
[null,"【屋面工程】分部小计"]
[null," 模板脚手架工程"]
[29,"模板","基础、梁、柱、板","m2"]
[30,"内脚手架","梁板支撑脚手架、抹灰脚手架","m2"]
[31,"外脚手架","双排钢管脚手架（含挂外网）","m2"]
[null,"【模板脚手架工程】分部小计"]
[null," 其他工程"]
[32,"散水","1.垫层材料种类:原土夯实\n2.混凝土种类:商品混凝土\n3.混凝土强度等级:C15,20石,15厚","m2"]
[33,"化粪池","1.水泥成品化粪池\n2.尺寸：按图纸要求容量",1]
[null,"【其他工程】分部小计"]
[34,"临时卫生间安置"]
[35,"精益办公室墙体拆除","面积：2.9m*5.05m"]
[36,"精益办公室新增墙体","面积：2.9m*10.4m"]
[37,"精益办公室新增平开门","尺寸：0.9m*2m"]
[null,"【其他工程】分部小计"]
[38,"电线"]
[39,"照明灯具"]
[40,"开关、插座"]
[41,"水管及配件"]
[]
[null,"【水电工程】分部小计"]
[38,"以上直接费合计"]
[39,"管理费"]
[40,"利润"]
[41,"税金"]
[42,"总价"]